For 1990-2009 cars

## Fluid and Lubricant Recommendations Except Holden

Application | Fluid/Lubricant
--- | ---
Automatic Transaxle

- 1.6L DOHC (Aisin 81-40LE)

ESSO JWS 3309 or Total Fluid III G

- 1.8L, 2.0L DOHC (ZF 4HP16)

ESSO LT 71141 or Total ATF H50235

- 2.0L Diesel (Aisin 55-51 LE)

ESSO JWS 3309 US ATF

Automatic Transaxle Shift Linkage | Engine Oil
Brake Fluid and Clutch Fluid | DOT-3 or DOT-4
Clutch Linkage Pivot Points | Engine Oil
Engine Coolant

- 1.4L, 1.6L, 1.8L, 2.0L DOHC and 2.0L Diesel

Mixture of clean, drinkable water and DEX-COOL® or good quality ethylene glycol base antifreeze (year-round coolant)

Important: Do not mix types of coolant.

Engine Oil

- 1.4L, 1.6L, 1.8L and 2.0L DOHC

API SL (ILSAC GF-III) Grade SAE5W-30 (Hot Area--SAE10W-30)

- 2.0L Diesel

MB 229.31, ACEA C3 5W-40

Floor Shift Linkage Points | Engine Oil
Hood and Door Hinges Fuel Door Hinge Rear Compartment Lid Hinges | Engine Oil
Hood Latch Assembly

- Pivots and Spring Anchor

Engine Oil

- Release Pawl

Multipurpose type grease meeting requirements NLGI No. 1 or 2

Key Lock Cylinders | Silicone Lubricant
Manual Transaxle | SAE 75W-90
Manual Transaxle Shift Linkage | Multipurpose type grease meeting requirements NLGI No. 1 or 2
Power Steering System | DEXRON® III or DEXRON® IID
Weatherstrips | Silicone Grease

## Fluid and Lubricant Recommendations Holden

Application | Fluid/Lubricant
--- | ---
Automatic Transaxle | ESSO LT 71141
Automatic Transaxle Shift Linkage | Engine Oil
Brake Fluid and Clutch Fluid | DOT-4
Clutch Linkage Pivot Points | Engine Oil
Engine Coolant | DEX-COOL® or conforming to Holden specification number GM6277M
Engine Oil |

• | SAE 5W-30 or 10W-30

• | API SL or SM

• | ILSAC GF-3 or GF-4

Floor Shift Linkage Points | Engine Oil
Hood and Door Hinges Fuel Door Hinge Rear Compartment Lid Hinges | Engine Oil
Hood Latch Assembly

- Pivots and Spring Anchor

Engine Oil

- Release Pawl

Multipurpose type grease meeting requirements NLGI No. 1 or 2

Key Lock Cylinders | Silicone Lubricant
Manual Transaxle | SAE 75W-90
Manual Transaxle Shift Linkage | Multipurpose type grease meeting requirements NLGI No. 1 or 2
Power Steering System | DEXRON® III
Weatherstrips | Silicone Grease