For 1990-2009 cars

## Child Restraint Tether Anchor Replacement Four Door

### Removal Procedure

1. Remove child seat anchorage cover.
2. Remove bolt and the child seat anchorage.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the child seat anchorage with the bolt.

Tighten
Tighten the child seat anchorage bolt to 10 N·m (89 lb in).

2. Install the child seat anchorage cover.

## Child Restraint Tether Anchor Replacement Five Door

### Removal Procedure

1. Remove child seat anchorage cover.
2. Remove bolt and the child seat anchorage.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the child seat anchorage with the bolt.

Tighten
Tighten the child seat anchorage bolt to 10 N·m (89 lb in).

2. Install the child seat anchorage cover.

## Child Restraint Tether Anchor Replacement Wagon

### Removal Procedure

1. Remove child seat anchorage cover.
2. Remove bolt and the child seat anchorage.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the child seat anchorage with the bolt.

Tighten
Tighten the child seat anchorage bolt to 10 N·m (89 lb in).

2. Install the child seat anchorage cover.