For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the door glass. Refer to Front Side Door Window Replacement or to Rear Side Door Window Replacement .
3. Disconnect the electrical connector.
4. Remove the nuts and the window regulator.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the window regulator with the nuts.

Tighten
Tighten the window regulator nuts to 8 N·m (71 lb in).

2. Connect the electrical connector.
3. Install the door glass. Refer to Front Side Door Window Replacement or to Rear Side Door Window Replacement .
4. Connect the negative battery cable.