For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the screws.
3. Remove the lamp assembly.
4. Remove the lamp socket from the lamp housing.
5. Remove the bulb.

### Installation Procedure

1. Install a new bulb.
2. Install the lamp socket in the lamp housing.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the lamp assembly with the screws.

Tighten
Tighten the lamp assembly screws to 4 N·m (35 lb in).

4. Connect the negative battery cable.