For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Pry off the reading lamp lens.
3. Remove the screws and the reading lamp.
4. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the reading lamp with the screws.

Tighten
Tighten the reading lamp screws to 1.5 N·m (13 lb in).

3. Install the reading lamp lens.
4. Connect the negative battery cable.