For 1990-2009 cars

### Removal Procedure

1. Remove the front bucket seat from the vehicle. Refer to Front Seat Replacement - Bucket .
2. Remove the each seat trim.
3. Disconnect the electrical connectors.
4. Remove the bolts and the seatback.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the cushion onto the seat track.
2. Install the seat cushion with the nuts.

Tighten
Tighten the front seat cushion nuts to 12 N·m (106 lb in).

3. Install the seat trims.
4. Install the front seat in the vehicle. Refer to Front Seat Replacement - Bucket .