For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the floor console. Refer to Front Floor Console Replacement.
3. Disconnect the electrical switch connectors.
4. Remove the pinch nut from the shift control cable adjuster.
5. Remove the cable from the bracket.
6. Remove the bolts and the nuts holding the shift control assembly to the floor panel.
7. Remove the shift control assembly.

### Installation Procedure

1. Install the shift control assembly.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the bolts and the nuts holding the shift control assembly to the floor panel and tighten to 8 N·m (71 lb in).
3. Install the shift control cable onto the bracket.
4. Install the adjuster pinch nut to the cable and tighten to 8 N·m (71 lb in).
5. Connect the electrical switch connectors.
6. Install the floor console. Refer to Front Floor Console Replacement.
7. Connect the negative battery cable.