For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Place a drain pan or suitable container under the vehicle.
3. Disconnect the oil cooler hoses from the radiator.
4. Remove the oil cooler line assembly bolt from the transaxle.
5. Remove the oil cooler line assembly.
6. Replace the transaxle oil cooler line seals. Refer to Transmission Fluid Cooler Pipe Seal Replacement.

### Installation Procedure

1. Install the oil cooler line assembly to the transaxle.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the oil cooler line assembly bolt and tighten to 10 N·m (89 lb in).
3. Connect the oil cooler hoses to the radiator.
4. Lower the vehicle.
5. Add fluid to the transaxle.
6. Check the fluid level.