For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the intake air tube.
3. Disconnect the breather hose.
4. Disconnect the coolant hose from the throttle body.
5. Disconnect the throttle cables by opening the release slot.
6. Disconnect the main throttle idle actuator (MTIA) electrical connector.
7. Remove the throttle body bolt and the nuts.
8. Remove the throttle body.

### Installation Procedure

1. Install the throttle body assembly to the intake manifold.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the throttle body retaining nuts and the bolt.

Tighten
Tighten the throttle body retaining nuts and the bolt to 15 N·m (11 lb ft).

3. Connect the throttle cable.
4. Connect the coolant hoses.
5. Connect the breather hose.
6. Install the intake air tube.
7. Connect the negative battery cable.