For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Door Hinge-to-Body Bolts | 36 N·m | 27 lb ft
Door Hinge-to-Door Bolts | 20 N·m | 15 lb ft
Door Hold-Open Link-to-Body Bolt | 25 N·m | 18 lb ft
Door Hold-Open Link-to-Door Bolts | 9 N·m | 80 lb in
Door Lock Striker Screws | 30 N·m | 22 lb ft
Door Pull Bracket Screws | 3 N·m | 27 lb in
Front Door Lock Screws | 8 N·m | 71 lb in
Inside Door Handle Screw | 3 N·m | 27 lb in
Outside Channel Molding Screw | 1.3 N·m | 12 lb in
Outside Door Handle Bolts | 4.5 N·m | 40 lb in
Power Folding Mirror Switch Bolt | 10 N·m | 89 lb in
Rear Door Guide Rail Bolts | 8 N·m | 71 lb in
Rear Door Guide Rail Screw | 4 N·m | 35 lb in
Rear Door Lock Screws | 8 N·m | 71 lb in
Window Regulator Nuts | 8 N·m | 71 lb in