For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Baffle Plate Attachment Bolts | 10 N·m | 89 lb in
Bearing Plate Bolts | 23.5 N·m | 17.5 lb ft
Damping Block Connection Bolt and Nut | 68 N·m | 50 lb ft
Engine-to-Transaxle Bolts (a) - Lower | 75 N·m | 55 lb ft
Engine-to-Transaxle Bolts (b) - Lower | 21 N·m | 15 lb ft
Engine-to-Transaxle Bolts (c) - Lower | 31 N·m | 23 lb ft
Fluid Filter Housing Cover Attachment Bolts | 10 N·m | 89 lb in
Fluid Level Plug | 45 N·m | 33 lb ft
Fluid Pan Connecting Bolts | 6 N·m | 53 lb in
Fluid Pan Drain Plug | 45 N·m | 33 lb ft
Fluid Pump Connecting Bolts | 10 N·m | 89 lb in
Lines Pressure Plugs | 20 N·m | 15 lb ft
Oil Cooler Inlet Pipe Bolts | 35 N·m | 26 lb ft
Oil Cooler Outlet Pipe Bolts | 35 N·m | 26 lb ft
Park/Neutral Position Switch | 10 N·m | 89 lb in
Pressure Control Regulator Attachment Bolts | 6 N·m | 53 lb in
Rear Cover Attachment Bolts | 23.5 N·m | 17.5 lb ft
Selector Lever on Transaxle Case | 15 N·m | 11 lb ft
Shift Control Assembly Mounting Bolt Nut | 8 N·m | 71 lb in
Shift Control Cable Adjuster Pinch Nut | 8 N·m | 71 lb in
Shift Control Cable Adjustment Nut | 8 N·m | 71 lb in
Slotted Nut | 220 N·m | 162 lb ft
Solenoid Valve Attachment Bolts | 6 N·m | 53 lb in
Speed Sensor Attachment Bolts - Input | 8 N·m | 71 lb in
Speed Sensor Attachment Bolts - Output | 8 N·m | 71 lb in
Torque Converter Attachment Bolts | 45 N·m | 33 lb ft
Transaxle Mount Bracket Cage Bolt (a) - Left | 110 N·m | 81 lb ft
Transaxle Mount Bracket Cage Bolt (b) - Left | 65 N·m | 48 lb ft
Transaxle Mount Bracket Cage Bolt (c) - Left | 65 N·m | 48 lb ft
Transaxle Mounting Bolts - Left | 48 N·m | 35 lb ft
Transaxle Mounting Bracket Bolts - Rear | 62 N·m | 45 lb ft
Transaxle-to-Engine Bolts - Upper | 75 N·m | 55 lb ft
Valve Body Bolts | 8 N·m | 71 lb in
Valve Body Upper and Lower Fixing Bolts | 6 N·m | 53 lb in
Valve Housing 1 Cover Attachment Bolts | 6 N·m | 53 lb in