For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (I/P). Refer to Instrument Panel Assembly Replacement in Instrument Panel, Gages, and Console.
2. Remove the nuts from the brace.
3. Remove the brake pedal.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the brace with nuts.

Tighten
Tighten the brace with nuts to 22 N·m (16 lb ft).

2. Install the brake pedal.
3. Install the I/P. Refer to Instrument Panel Assembly Replacement in Instrument Panel, Gages, and Console.