For 1990-2009 cars

### Removal Procedure

1. Remove the door seal trim. Refer to Door Water Deflector Replacement .
2. Disconnect the outside door handle lock rod.
3. Remove the bolt and the lock cylinder.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the lock cylinder with the bolt.

Tighten
Tighten the outside door handle bolt to 4.5 N·m (40 lb in).

2. Connect the outside door handle lock rod.
3. Install the door seal trim. Refer to Door Water Deflector Replacement .