For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the front wheel well splash shields. Refer to Wheelhouse Splash Shield Replacement .
3. Remove the fog lamps and the headlamps. Refer to Front Fog Lamp Replacement and Headlamp Replacement .
4. Remove the fender-to-fascia bolts and the screws.
5. Remove the lower fascia screws and the bolts.
6. Remove the upper fascia screws.
7. Remove the front bumper fascia.

### Installation Procedure

1. Install the front bumper fascia.
2. Install the upper fascia screws.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the lower fascia screws and the bolts.

Tighten
Tighten the lower fascia screws to 2 N·m (18 lb in).

4. Install the fender-to-fascia bolts and the screws.

#### Tighten

• | Tighten the fender-to-fascia bolts to 10 N·m (89 lb in).

• | Tighten the fender-to-fascia screws to 2 N·m (18 lb in).

5. Install the headlamps and the fog lamps. Refer to Headlamp Replacement and Front Fog Lamp Replacement .
6. Install the front wheel well splash shields. Refer to Wheelhouse Splash Shield Replacement .
7. Connect the negative battery cable.