For 1990-2009 cars

### Removal Procedure

1. Remove the outside channel molding. Refer to Outer Belt Sealing Strip Replacement .
2. Position the weatherstrip in order to access the screws.
3. Remove the screws and the center pillar molding.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the screws and the center pillar molding.

Tighten
Tighten the center pillar molding screws to 1.3 N·m (12 lb in).

2. Install the weatherstrip to its original position.
3. Install the outside channel molding. Refer to Outer Belt Sealing Strip Replacement .