For 1990-2009 cars

#### Special Tools

J 28467-B (DW117) Universal Engine Support Fixture

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Remove the battery.
2. Install J 28467-B (1).
3. Remove the left transaxle mounting bolts.
4. Remove the cage bolts (1, 3) and nut (2) from the left transaxle mounting bracket.
5. Remove the mounting bracket.

### Installation Procedure

1. Install the left transaxle mounting bracket.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the cage bolts (1, 3) and nut (2) to the mounting bracket and tighten..

• | bolt (3) to 110 N·m (81 lb ft)

• | bolt (1) to 65 N·m (48 lb ft)

• | nut (2) to 65 N·m (48 lb ft)

3. Install the left transaxle mounting bolts and tighten to 48 N·m (35 lb ft).
4. Remove J 28467-B (1).
5. Install the battery.