For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
compressor | V5
Evaporator

- Capacity

8.7 kg/min

19.2 lbs/min

- Airflow Rate

6000±10%

Receiver-Dryer | AL R/Drier
Refrigerant

- Type

R-134a System

- Capacity - Left Hand Drive

640 g

1.4 lbs

- Capacity - Right Hand Drive

680 ± 20

1.5 lbs

Refrigerant Oil in A/C System

- Type

Union Carbide 488 PAG OIL

- Capacity

220 ml

7.4 oz