For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

Important: Operate the automatic temperature control system and rotate the temperature control knob until the temperature reaches to the maximum.

1. Disconnect the negative battery cable.
2. Remove the glove box lower panel cover. Refer to Instrument Panel Storage Compartment Replacement in Instrument Panel, Gages and Console.
3. Disconnect the electrical connector.
4. Remove the actuating rod by snapping it out of the lever with needle-nose pliers.
5. Remove the motor retaining screws.
6. Remove the temperature door motor.

### Installation Procedure

1. Install the temperature door motor with the retaining screws.
2. Install the actuating rod onto the lever.
3. Connect the electrical connector.
4. Install the glove box. Refer to Instrument Panel Storage Compartment Replacement in Instrument Panel, Gages and Console.
5. Connect the negative battery cable.