For 1990-2009 cars

## Instrument Cluster Trim Panel Replacement Four Door

### Removal Procedure

1. Remove the screws and the instrument cluster trim panel.
2. Disconnect the electrical connectors.

### Installation Procedure

1. Connect the electrical connectors.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the instrument cluster trim panel with the screws.

Tighten
Tighten the instrument cluster trim panel screws to 4 N·m (35 lb in).

## Instrument Cluster Trim Panel Replacement Five Door/Wagon

### Removal Procedure

1. Remove the screws from the instrument cluster trim panel.
2. Remove the instrument cluster trim panel.

### Installation Procedure

1. Install the instrument cluster trim panel.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the instrument cluster trim panel screws.

Tighten
Tighten the instrument cluster trim panel screws to 4 N·m (35 lb in).