For 1990-2009 cars

## Fastener Tightening Specifications Gasoline Engines

Application | Specification
--- | ---
Metric | English
Catalytic Converter-to-Exhaust Manifold Nuts | 40 N·m | 30 lb ft
Catalytic Converter-to-Underbody Shield | 2.5 N·m | 22 lb in
Exhaust Front Pipe-to-Catalytic Converter Nuts | 40 N·m | 30 lb ft
Exhaust Front Pipe-to-Front Muffler | 30 N·m | 22 lb ft
Exhaust Manifold Cover Bolts | 15 N·m | 11 lb ft
Front Bracket-to-Cylinder Block Bolt | 50 N·m | 37 lb ft
Front Muffler-to-Rear Muffler Nuts | 30 N·m | 22 lb ft
Front Muffler-to-Underbody Shield | 2.5 N·m | 22 lb in
Rear Muffler-to-Underbody Shield | 2.5 N·m | 22 lb in