For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the fuel rail. Refer to Fuel Injection Fuel Rail Assembly Replacement .
3. Disconnect the manifold absolute pressure (MAP) sensor connector from the MAP sensor.
4. Remove the MAP sensor retaining bolt.
5. Remove the MAP sensor from the intake manifold.

### Installation Procedure

1. Connect the MAP sensor connector to the MAP sensor.
2. Install the MAP sensor into the intake manifold.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the MAP sensor retaining bolt.

Tighten
Tighten the MAP sensor retaining bolt to 8 N·m (71 lb in).

4. Connect the fuel rail. Refer to Fuel Injection Fuel Rail Assembly Replacement .
5. Connect the negative battery cable.