For 1990-2009 cars

## Engine Cooling System Specifications 1.4L DOHC/1.6L DOHC

Application | Specification
--- | ---
Metric | English
Cooling Type | Forced Water Circulation
Radiator Type | Cross-flow
Water Pump Type | Centrifugal
Thermostat Type | Pellet Type
Coolant Capacity | 7.2 L | 7.6 qt

## Engine Cooling System Specifications 1.8L DOHC

Application | Specification
--- | ---
Metric | English
Cooling Type | Forced Water Circulation
Radiator Type | Cross-flow
Water Pump Type | Centrifugal
Thermostat Type | Pellet Type

## Engine Cooling System Specifications 2.0L DOHC

Application | Specification
--- | ---
Metric | English
Cooling Type | Forced Water Circulation
Radiator Type | Cross-flow
Water Pump Type | Centrifugal
Thermostat Type | Pellet Type
Coolant Capacity | 7.5 L | 7.9 qt

## Engine Cooling System Specifications 2.0L Diesel

Application | Specification
--- | ---
Unit | Standard
Cooling System
Cooling Type | -- | Forced Water Pressurized
Coolant

- Type

--

DEX-COOL/Silicated Based Coolant

- Capacity

L (qt)

8 (8.5)

Thermostat

- Type

--

Wax Pallet

- Temperature (Opened Initially)

°C (°F)

78-82°C (172-180°F)

- Temperature (Completely Open)

°C (°F)

95°C (203°F)

- Temperature (Completely Closed)

°C (°F)

75°C (167°F)

Cooling Fan

- Fan

--

Axial Flow Type

- Number of Blades

EA

7

- Diameter

mm (in)

408 mm (16.06 in)

- ON Temperature at Low Speed

°C (°F)

94°C (201°F)

- OFF Temperature at Low Speed

°C (°F)

91°C (195°F)

- ON Temperature at High Speed

°C (°F)

98°C (208°F)

- OFF Temperature at High Speed

°C (°F)

95°C (203°F)

Surge Tank

- Open Pressure of the Pressure Valve

kPa/psi

140 (20)

- Open Pressure of the Vacuum Valve

kPa/psi

10 (1.5)

Water Pump

- Type

--

Centrifugal

- Impeller Diameter

mm (in)

85 mm (3.35 in)

- Number of Impeller Blades

EA

7

Radiator

- Type

mm (in)

Cross Flow

- Core Width

mm (in)

565 mm (22.24 in)

- Core Height

mm (in)

414 mm (16.3 in)

- Core Depth

mm (in)

27 mm (1.063 in)