For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Pry off the interior courtesy lamp lens.
3. Remove the screws and the switch.
4. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the sunroof control switch with the screws.

Tighten
Tighten the power sunroof control switch screws to 2 N·m (18 lb in).

3. Install the interior courtesy lamp lens.
4. Connect the negative battery cable.