For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the glove box. Refer to Instrument Panel Storage Compartment Replacement .
3. Remove the actuating rod by snapping the rod out of the lever with needle-nose pliers.
4. Disconnect the electrical connector.
5. Remove a screw and the bracket mounting high-blower relay.
6. Remove the motor retaining screws.
7. Remove the motor.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the motor with the retaining screws.
2. Install the actuating rod.
3. Connect the electrical connector.
4. Install the bracket mounting high-blower relay with a screw.
5. Remove the glove box. Refer to Instrument Panel Storage Compartment Replacement .
6. Connect the negative battery cable.