For 1990-2009 cars

### Removal Procedure

Caution: Refer to Sensing and Diagnostic Module Voltage after Ignition is Turned Off Caution in the Preface section.

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the glove box. Refer to Instrument Panel Storage Compartment Replacement .
3. Disconnect the passenger air bag yellow electrical connector.
4. Remove the instrument panel (I/P) module by removing the mounting bolts from the air bag bracket.

### Installation Procedure

1. Install the I/P module to the I/P.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the I/P module mounting bolts.

Tighten
Tighten the I/P module mounting bolts to 11 N·m (97 lb in).

3. Connect the passenger air bag yellow electrical connector.
4. Install the glove box. Refer to Instrument Panel Storage Compartment Replacement .
5. Connect the negative battery cable.