For 1990-2009 cars

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation .
3. Inspect the brake pads for wear.
4. Measure the thickness.

Specification

• | The minimum thickness of the inner or the outer front pad is 2 mm (0.08 in).

• | The minimum thickness of the inner or the outer rear pad is 2 mm (0.08 in).

5. Install the brake pads in axle sets only.
6. Install the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation .
7. Lower the vehicle.