For 1990-2009 cars

### Removal Procedure

1. Remove the door seal trim. Refer to Door Water Deflector Replacement.
2. Remove the center pillar molding. Refer to Center Pillar Applique Replacement.
3. Remove the screws that secure the glass to the window regulator.
4. Remove the glass from the door.

### Installation Procedure

1. Install the glass in the door and position the glass within the window regulator.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the glass to the window regulator with the screws.

Tighten
Tighten the glass screws to 7 N·m (62 lb in).

3. Install the center pillar molding. Refer to Center Pillar Applique Replacement.
4. Install the door seal trim. Refer to Door Water Deflector Replacement.