For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the engine cover.
3. Disconnect the sensor electrical connector.
4. Remove the timing belt front cover. Refer to Timing Belt Replacement .
5. Remove the camshaft position sensor bolts.
6. Remove the camshaft position sensor from the top.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the camshaft position sensor and bolts.

Tighten
Tighten the camshaft position bolts to 8 N·m (71 lb in).

2. Install the timing belt front cover, the crankshaft pulley, the accessory drive belt, and the air filter.
3. Connect the sensor electrical connector.
4. Install the engine cover.
5. Connect the negative battery cable.