For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the rod clamp. Refer to Shift Linkage Adjustment .
3. Remove the console.
4. Remove the gearshift lever housing bolts and the gearshift lever housing.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the gearshift lever housing and the gearshift lever housing bolts.

Tighten
Tighten the gearshift housing bolts to 7 N·m (62 lb in).

2. Adjust the shift linkage.
3. Install the console.
4. Connect the negative battery cable.