For 1990-2009 cars

### Removal Procedure

1. Remove the front seat belt bolt and washer.
2. For driver seat belt buckle, remove the electrical connector.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the front seat belt bolt and washer.

Tighten
Tighten the front seat belt bolt to 42 N·m (31 lb ft).

2. For driver seat belt buckle, connect the electrical connector.