For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the electronic ignition (EI) system ignition coil connector.
3. Note the ignition wire location and remove the ignition wires.
4. Remove the EI system ignition coil retaining bolts.
5. Remove the EI system ignition coil.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the EI system ignition coil into the mounting location and install the retaining bolts.

Tighten
Tighten the EI system ignition coil retaining bolts to 10 N·m (89 lb in).

2. Connect the EI system ignition coil connector.
3. Install the ignition wires.
4. Connect the negative battery cable.