For 1990-2009 cars

1. Remove the transaxle from the vehicle. Refer to Transmission Replacement .
2. Remove the shift lever cover bolts and the shift lever cover. Do not disassemble the shift lever cover.
3. Remove the transaxle cover bolts and the transaxle cover.
4. Remove the bearing plate bolts and the bearing plate, with the shafts attached. Do not disassemble the shafts.
5. Remove the differential from the transaxle housing. Do not disassemble the differential. Refer to Differential Case Disassemble .
6. Remove the backup lamp switch from the transaxle housing.
7. Remove the clutch-release bearing and the clutch-release bearing guide. Refer to Clutch Concentric Actuator Cylinder Replacement .
8. Remove the speedometer-driven gear bolt and the speedometer-driven gear from the transaxle housing.