For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accessory Mounting Bracket Bolts | 37 N·m | 27 lb ft
Air Cleaner Element Cover Screw | 2 N·m | 187 lb in
Air Cleaner Housing Bolts | 10 N·m | 89 lb in
Camshaft Position Sensor Bolts | 8 N·m | 71 lb in
CO Potential Mounting Bolt | 8 N·m | 71 lb in
Controlled Canister Purge Solenoid Bracket Bolt | 5 N·m | 44 lb in
Crankshaft Position (CKP) Sensor Retaining Bolt | 8 N·m | 71 lb in
Electronic Ignition (EI) System Ignition Coil Retaining Bolts | 10 N·m | 89 lb in
Engine Control Module (ECM) Bolts | 4 N·m | 35 lb in
Engine Control Module (ECM) Retaining Nuts | 8 N·m | 71 lb in
Engine Coolant Temperature (ECT) Sensor Bolt | 20 N·m | 15 lb ft
Evaporative Emission (EVAP) Canister Flange Bolt | 4 N·m | 35 lb in
Evaporative Emission (EVAP) Canister Purge Solenoid Bracket Bolt | 5 N·m | 44 lb in
Evaporative Emission (EVAP) Canister Vent Solenoid Valve Bracket Belt Nuts | 8 N·m | 71 lb in
Exhaust Gas Recirculation (EGR) Valve Retaining Bolts | 30 N·m | 22 lb ft
Fuel Filter Mounting Bracket Assembly Bolt | 4 N·m | 35 lb in
Fuel Filter Mounting Bracket Bolts | 4 N·m | 35 lb in
Fuel Pressure Regulator Retaining Bolt | 12 N·m | 106 lb in
Fuel Rail Retaining Bolts | 25 N·m | 18 lb ft
Fuel Tank Retaining Bolts | 20 N·m | 15 lb ft
Idle Air Control Valve Retaining Bolts | 3 N·m | 27 lb in
Intake Air Temperature (IAT) Sensor | 20 N·m | 15 lb ft
Knock Sensor Bolt | 20 N·m | 15 lb ft
Manifold Absolute Pressure (MAP) Sensor Retaining Bolt | 4 N·m | 35 lb in
Oxygen Sensor Bolt | 44 N·m | 33 lb ft
Rear A/C Compressor Mounting Bracket Bolts | 35 N·m | 26 lb ft
Spark Plug Cover Bolts | 3 N·m | 27 lb ft
Throttle Body Retaining Nuts | 10 N·m | 89 lb in
Throttle Position Sensor Retaining Bolts | 2 N·m | 18 lb in