For 1990-2009 cars

### Removal Procedure

1. Remove the engine cover.
2. Remove the air cleaner housing bolts.
3. Loosen the clamps.
4. Remove the breather tube from the camshaft cover.
5. Remove the air cleaner housing.

### Installation Procedure

1. Install the air cleaner housing.
2. Tighten the clamps.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the air cleaner housing bolts.

Tighten
Tighten the air cleaner housing bolts to 10 N·m (89 lb in).

4. Install the engine cover.
5. Connect the negative battery cable.