For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Cleaner Housing Bolts | 10 N·m | 89 lb in
Automatic Tensioner Bolt | 25 N·m | 18 lb ft
Camshaft Bearing Bridge and Oil Pan Scraper Bolts | 20 + 45° | 15 + 45°
Camshaft Bearing Cap Bolts | 8 N·m | 71 lb in
Camshaft Cover Bolts | 8 N·m | 71 lb in
Charcoal Canister Purge and Exhaust Gas Recirculation Solenoid Bracket Bolt | 5 N·m | 44 lb in
Connecting Rod Bearing Cap Bolts | 35 + 45° + 15° N·m | 26 + 45° + 15° lb ft
Coolant Bypass Housing and Mounting Bolts | 15 N·m | 11 lb ft
Crankshaft Bearing Cap Bolts | 50 + 45° + 15° N·m | 37 + 45° + 15° lb ft
Crankshaft Gear Bolt | 145 + 30° + 15° N·m | 107 + 30° + 15° lb ft
Crankshaft Pulley Bolts | 20 N·m | 15 lb ft
Cylinder Head Bolts | 25+ 90° + 90° + 90° N·m | 18 + 90° + 90° + 90° lb ft
Direct Ignition System Coil and Exhaust Gas Recirculation Mounting Bracket Bolts | 25 N·m | 18 lb ft
Engine Mount Bracket Retaining Bolts and Nuts | 55 N·m | 41 lb ft
Engine Mount Retaining Bolts | 45 N·m | 33 lb ft
Engine-to-Intake Manifold Support Bracket Bolts | 20 N·m | 15 lb ft
Exhaust Camshaft Gear Bolt | 50 + 60° + 15° N·m | 37 + 60° + 15° lb ft
Exhaust Flex Pipe-to-Catalytic Converter to Connecting Pipe Retaining Nuts | 35 N·m | 26 lb ft
Exhaust Flex Pipe-to-Exhaust Manifold Retaining Nuts | 35 N·m | 26 lb ft
Exhaust Manifold Heat Shield Bolts | 8 N·m | 71 lb in
Exhaust Manifold Retaining Nuts | 22 N·m | 16 lb ft
Flex Plate Bolts | 45 N·m | 33 lb ft
Flywheel Bolts | 65 + 30° + 15° N·m | 48 + 30° + 15° lb ft
Front Timing Belt Cover Bolts | 6 N·m | 53 lb in
Generator-to-Intake Manifold Strap Bracket Bolt | 22 N·m | 16 lb ft
Generator-to-Intake Manifold Support Bracket Bolts | 37 N·m | 27 lb ft
Intake Camshaft Gear Bolt | 50 + 60° + 15° N·m | 37 + 60° + 15° lb ft
Intake Manifold Retaining Bolt and Nuts | 22 N·m | 16 lb ft
Intake Manifold Support Bracket Lower Bolt | 25 N·m | 18 lb ft
Intake Manifold Support Bracket Upper Bolts | 25 N·m | 18 lb ft
Lower Block Support Bracket and Splash Shield Bolts | 35 N·m | 26 lb ft
Oil Pan Drain Plug | 35 N·m | 26 lb ft
Oil Pan Flange-to-Transaxle Bolts | 40 N·m | 30 lb ft
Oil Pan Retaining Bolts | 10 N·m | 89 lb in
Oil Pressure Switch | 40 N·m | 30 lb ft
Oil Pump Rear Cover Bolts | 6 N·m | 53 lb in
Oil Pump Retaining Bolts | 10 N·m | 89 lb in
Oil Suction Pipe Bolts | 8 N·m | 71 lb in
Oil Suction Pipe Support Bracket Bolts | 16 N·m | 53 lb in
Pulse Pickup Sensor Disc | 13 N·m | 10 lb ft
Rear Timing Belt Cover Bolts | 7 N·m | 62 lb ft
Safety Relief Valve Bolt | 30 N·m | 22 lb ft
Spark Plug Cover Bolts | 8 N·m | 71 lb ft
Spark Plugs | 20 N·m | 15 lb ft
Thermostat Housing Mounting Bolts | 15 N·m | 11 lb ft
Throttle Cable Bracket Bolts | 8 N·m | 71 lb in
Timing Belt Automatic Tensioner Bolts | 25 N·m | 18 lb ft
Timing Belt Idler Pulley Bolt | 25 N·m | 18 lb ft
Timing Belt Idler Pulley Nut | 25 N·m | 18 lb ft
Transaxle Bell Housing Bolts | 75 N·m | 55 lb ft
Transaxle Torque Converter Bolts | 60 N·m | 44 lb ft