For 1990-2009 cars

#### Special Tools

• | EN-48253 Accessory Belt Remover/Installer

• | EN-48300 Tensioner Remover/Installer

• | EN-48952 Tensioner Spring Holding Pin

### Removal Procedure

1. Remove the engine cover. Refer to Engine Cover Replacement .
2. Raise and suitably support the vehicle.
3. Remove the right front wheel. Refer to Tire and Wheel Removal and Installation .
4. Remove the engine front shield at the position of right front wheel.
5. Install the EN-48253 onto the tensioner lever guide and rotate the tensioner at clockwise.
6. Rotate the tensioner fully and simultaneously insert EN-48952 to the tensioner pin hole.
7. Remove the accessory belt.

### Installation Procedure

1. Install the accessory belt.
2. Install the EN-48253 to the tension lever guide and rotate the tensioner counterclockwise.

Notice: Refer to Fastener Notice in the Preface section.

Important: The tensioner dowel pin (1) is inserted into the tensioner dowel pin hole (2).

3. Install the tensioner using EN-48300 .

Tighten
Tighten the tensioner retaining bolt to 48 N·m (35.4 lb ft).

4. Remove EN-48952 using EN-48253 .
5. Install the right front engine shield.
6. Install the right front tire.
7. Lower the vehicle.
8. Install the engine cover. Refer to Engine Cover Replacement .