For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement and to Rear Door Trim Panel Replacement .
2. Remove the door seal trim.

### Installation Procedure

1. Install the door seal trim.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the door trim panel. Refer to Front Side Door Trim Panel Replacement and to Rear Door Trim Panel Replacement .