For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the rear trailing link-to-rear knuckle nut.
3. Remove the rear trailing link-to-trailing link bracket nut and the rear trailing link-to-knuckle bolt.
4. Remove the rear trailing link.

### Installation Procedure

1. Install the rear trailing link.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the rear trailing link bracket nut and the bolt.

Tighten
Tighten the rear trailing link-to-trailing link bracket nut to 100 N·m (74 lb ft).

3. Install the trailing link-to-knuckle nut.

Tighten
Tighten the rear trailing link-to-knuckle nut to 150 N·m (111 lb ft).

4. Lower the vehicle.