For 1990-2009 cars

#### Special Tools

DT 46474 (DW260-060) Brake F Cup Spring Compressor

Warning: Refer to Safety Glasses Warning in the Preface section.

1. Remove the side shaft. Refer to Side Shaft Removal.
2. Remove the disc set.
3. Remove the brake F inner disc carrier.
4. Install DT 46474 (1) and remove the brake F split stop ring.
5. Remove DT 46474 (1).
6. Remove the cup spring.
7. Release the piston F by applying compressed air to the bore.

Note: Remove the plate by pressing the plate upward from beneath.

8. Remove piston F and remove the bearing plate with the spur gear.