For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the front left wheel. Refer to Tire and Wheel Removal and Installation .
3. Remove the bolts and the screws and the front wheel well splash shield.
4. Disconnect the washer hose from the washer pump.
5. Disconnect the reservoir pump electrical connectors.
6. Remove the bolts and the reservoir.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the reservoir with the bolts.

Tighten
Tighten the washer fluid reservoir bolts to 8 N·m (71 lb in).

2. Connect the reservoir pump electrical connector.
3. Connect the washer hose to the washer pump.
4. Install the front wheel well splash shield with the bolts and screws.

Tighten
Tighten the front wheel well splash shield bolts to 1.5 N·m (13 lb in).

5. Install the front left wheel. Refer to Tire and Wheel Removal and Installation .
6. Connect the negative battery cable.