For 1990-2009 cars

## Clock Replacement Five Door/Wagon

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the instrument panel center upper cover.
3. Remove the screws and digital clock.
4. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the digital clock with the screws.

Tighten
Tighten the screws to 3 N·m (27 lb in).

3. Install the center molding.
4. Connect the negative battery cable.

## Clock Replacement Four Door

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the Instrument panel center molding. Refer to Instrument Panel Center Trim Panel Replacement .
3. Disconnect the electrical connector.
4. Remove the screws and digital clock.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the digital clock with the screws.
2. Connect the electrical connector.
3. Install the Instrument panel center molding. Refer to Instrument Panel Center Trim Panel Replacement .
4. Connect the negative battery cable.