For 1990-2009 cars

Notice: Refer to Fastener Notice in the Preface section.

1. Install the line pressure measurement plug.

Tighten
Tighten the plug to 20 N·m (15 lb ft).

2. Install the baffle plate and the baffle plate bolts.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

3. Install the oil filter and the oil filter bolt.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

4. Install the paper gasket.
5. Install the metal gasket.
6. Install the torque converter housing.
7. Install the torque converter bolts and hand tighten in the following order: 7, 20, 12, 16, and 4.
8. Final tighten the bolts.

Tighten
Tighten the bolts to 15 N·m (11 lb ft).

9. Hand tighten the remaining bolts in the following order: 15, 3, 14, 5, 13, 22, 11, 21, 10, 9, 19, 8, 18, 17, 6, 1, and 2.
10. Final tighten all the bolts.

Tighten
Tighten the bolts to 23 N·m (17 lb ft)