For 1990-2009 cars

### Removal Procedure

1. Lower the rear seat back.
2. Remove the rear quarter upper trim panel.
3. Remove the rear seat belts. Refer to Shoulder Belt Replacement - Rear .
4. Remove the child seat anchorage. Refer to Child Restraint Tether Anchor Replacement .
5. Remove the plastic retaining clips and the deck lid sill plate cover.

### Installation Procedure

1. Install the rear deck lid sill plate cover with the plastic retaining clips.
2. Install the child seat anchorage. Refer to Child Restraint Tether Anchor Replacement .
3. Install the rear seat belts. Refer to Shoulder Belt Replacement - Rear .
4. Install the rear quarter upper trim panel.
5. Raise the rear seat.