For 1990-2009 cars

### Removal Procedure

1. Lower the window completely.
2. Remove the outside channel molding screw.
3. Lift the outside channel molding off the door.

### Installation Procedure

1. Press the outside channel molding onto the door.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the outside channel molding screw.

Tighten
Tighten the outside channel molding screw to 1.3 N·m (12 lb in).

3. Raise the window.