For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the headliner. Refer to Headlining Trim Panel Replacement .
3. Remove the drain hoses.
4. Disconnect the electrical connectors.
5. Remove the screws and the motor.
6. Remove the motor control module.
7. Remove the bolts and the housing from the vehicle.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the housing to the roof of the vehicle with the bolts.

Tighten
Tighten the sunroof housing bolts to 10 N·m (89 lb in).

2. Install the motor control module.
3. Install the motor with the screws.

Tighten
Tighten the sunroof motor screws to 3 N·m (27 lb in).

4. Connect the electrical connectors.
5. Install the drain hoses.
6. Install the headliner. Refer to Headlining Trim Panel Replacement .
7. Connect the negative battery cable.