For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the rain sensor cover.
3. Disconnect the electrical connector.
4. Remove the rain sensor.

### Installation Procedure

1. Install the rain sensor.
2. Connect the electrical connector.
3. Install the rain sensor cover.
4. Connect the negative battery cable.