For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the upper and the lower steering column cover panel screws.
3. Remove the upper and the lower steering column cover panels.
4. Remove the turn signal switch by pushing the tabs on the top and the bottom of the switch housing.
5. Disconnect the electrical connections from the turn signal switch.

### Installation Procedure

1. Connect the electrical connections to the turn signal switch.
2. Install the turn signal switch by snapping it into the switch housing.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the upper and the lower steering column cover panels. Install the upper and the lower steering column cover panel screws and tighten to 2.5 N·m (22 lb in).
4. Connect the negative battery cable.