For 1990-2009 cars

#### Special Tools

DW-110-060 Engine Assembly Support Fixture

### Removal Procedure

Note: Only lift the engine far enough to take the weight off the transaxle rear mount assembly, or damage to the mount and lifting equipment failure may occur.

1. Support the engine assembly using DW-110-060 .
2. Remove the engine shield.
3. Remove the front crossmember.
4. Remove the engine rear mount from the transaxle.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the engine rear mount to the transmission.

Tighten
Tighten the engine rear mount retaining bolts to 90 N·m (66 lb ft).

2. Install the front crossmember.
3. Install the engine shield.
4. Remove the engine support fixture DW-110-060 .