For 1990-2009 cars

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
1 |

1. Turn the ignition ON.
2. Measure the voltage at the wiper motor connector terminal 8.

Is the voltage within the specified range.

11-14 V

Go to Step 3

Go to Step 2

2 | Repair the open circuit between the wiper motor connector terminal 8 and fuse F9. Did you complete the repair? | -- | System OK | --
3 | Replace the wiper motor. Did you complete the replacement? | -- | System OK | --