For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Compressor | V5
Evaporator

- Capacity

8.7 kg/min

19.2 lbs/min

- Airflow Rate

6000±10%

Receiver-Dryer | AL R/Drier
Refrigerant

- Type

R-134a System

- Capacity - Left Hand Drive

670g ± 20

1.5 lbs

- Capacity - Right Hand Drive

720g ± 20

1.6 lbs

Refrigerant Oil in A/C System

- Type

ISUPAG 513

- Capacity

175 ml

5.9 oz